Date:	February 4, 1998

Objectives:

Continue to search for an appropriate hydride material and find all applicable pricing for a commercial hydride storage system.

Find out where the Biology store is located.

Design entrapment filters for the product water collection and decide what size the collection size should be.

Procedure Utilized:

Environment:

Temperature-	NA

Barometer-	NA

Relative Humidity-	NA

Results & Conclusions:

W.L. Gore is going to provide some 50 cm2 membrane and electrode assemblies for testing. I have aquired a test fixture for the electrolyzer. The catalyst will be a Ti mesh with platnium for the anode side and Pt on carbon on the cathode side of the reaction. The Idea being that the Ti and Pt mesh will provide a stable oxidative surface for the reaction to take place and the membrane will only allow the hydrogen to cross the membrane.