Date:	February 5, 1998

Objectives:

Continue to search for an appropriate hydride material and find all applicable pricing for a commercial hydride storage system.

Finish collection entrapment vessel design for the product water collection and decide what size the collection size should be.

Procedure Utilized:

Environment:

Temperature-	NA

Barometer-	NA

Relative Humidity-	NA

Results & Conclusions:

W.L. Gore is going to provide some 50 cm2 membrane and electrode assemblies for testing. I have acquired a test fixture for the electrolyzer. The trap will be a collection system that will prevent the introduction of air or any other contaminants into the water. I will have to discard the original samples until the system has reached a steady state, however for curiosity sake the samples will be saved as a startup analysis for regenerative systems.