Date:	February 13, 1998

Objectives:

Collect literature about the construction of a proton exchange membrane Electrolyzer.

Procedure Utilized:

Literature Search

Environment:

Temperature-	NA

Barometer-	NA

Relative Humidity-	NA

Results & Conclusions:

Dr. S. Srinivasan has suggested the use of an advanced design proton exchange membrane Electrolyzer that is documented in the the paper "An advanced design for a Proton Exchange Membrane Electrolyzer". Internation Journal of Hydrogen Energy. 1994

The electrolyzer is made from Nafion membrane approximately 115 in thickness and Ti mesh that is plated with Platnium. The Ti mesh is then sprayed with an electrolyte (Nafion) for the purpose of conduction.